	Form Factor (Midi, Micro, Mini , Full)
	MICRO

	Chassis
	SPCC  :0.4mm

	
	
	

	PSU Form Factor
	Bottom/ATX
	

	M/B Form Factor
	M-ATX、ITX
	

	Front Panel
	ABS，MESH
	

	Top Panel
	metal cover
	

	Branding
	Box
	
	

	
	Unit
	
	

	
	(Unit) Position
	
	

	Side Panel
	Left
	Tempered Glass
	

	
	Right
	metal cover
	

	External Drive Bay(s)
	5.25" (ODD)
	*0
	

	
	3.5"
	*0
	

	Internal Drive Bay(s)
	3.5" (HDD)
	1*3.5HDD+5*2.5SSD  or  2*3.5HDD+3*2.5SSD or 3*3.5HDD+2*2.5SSD  or 2*3.5HDD+2*2.5SSD
	

	
	2.5" (SSD)
	
	

	
	
	

	I/O
	Buttons
	*2
	

	
	USB1.1 Port(s)
	*0
	

	
	USB2.0 Port(s)
	*1
	

	
	USB3.0 Port(s)
	*1
	

	
	USB3.1 Port(s)
	*0
	

	
	HD Audio Support
	Combo Audio(CTIA)*1
	

	
	Type C
	*1(2.)
	

	
	P-Lock
	*1 
	

	
	RGB Controller
	*0 
	

	
	Controller max. fans
	*0                                 
	

	
	RGB Controller max. LED strips
	*0                             
	

	
	Remote (IR or RF)
	*0
	

	Cooling Fan  Support
	Front
	2x120mm(Fan include),2x140mm(Fan optional)
	

	
	Top
	2x120mm(Fan include) ,2x140mm (Fan optional)
	

	
	Rear
	1x120mm(Fan include)
	

	
	Left Side
	0
	

	
	PSU Cover
	2x120mm (Fan optional)
	

	Water Cooling Support
(Radiator Size)
	Front
	120mm, 140mm,240mm,280mm.360mm
	

	
	Top
	120mm, 140mm,240mm
	

	
	Rear
	120mm*1
	

	Dust Cover
	Bottom  and top cover with dust filter
	

	Slots
	*5
	

	Carton & Logo
	GAMEMAX
	

	Dimensions
	Chassis
	(L)340*(W)200*(H)436mm
	

	
	Full Case (inc Fascia)
	(L)386*(W)205*(H)449mm
	

	
	Carton
	(L)486*(W)255*(H)433mm
	

	
	Net Weight (Kg)
	kgs
	

	
	Gross Weight (Kg)
	kgs
	

	VGA Card Length
	up to 330mm
	

	CPU Cooler Height
	155mm
	

	Cable Management Depth
	19mm
	

	PSU
	Included
	*0
	

	
	Wattage
	/
	

	
	80Plus Category
	/
	

	
	Rail Outputs
	/
	

	MOQ
	pcs
	




